<control> note_offset=1
<region> key=63 sample=*sine
<region> lokey=50 hikey=55 pitch_keycenter=50 sample=*sine
<region> lokey=40 hikey=44 pitch_keycenter=40 xfin_lokey=36 xfin_hikey=40 xfout_lokey=44 xfout_hikey=48 sample=*sine
<control> note_offset=-1
<region> key=63 sw_lokey=24 sw_hikey=28 sw_last=25 sw_up=25 sw_down=25 sw_previous=62 sample=*sine
<control> note_offset=1 octave_offset=1
<region> key=63 sample=*sine
<control> note_offset=-1 octave_offset=-1
<region> key=63 sample=*sine
<control> // Check that this does not reset either note or octave offset
<region> key=63 sample=*sine
